iQImplementationExampleExt

Flash Layout
Bootloader Start: 		0x08000000
Bootloader Size: 			14932B  
Bootloader Page Size: 		16000B
Config File Start: 		0x08004000
Main Start: 			0x08004400
Main Page Size: 			40000B
User Flash Start:		0x0800E400	
User Flash Pages:			 5000B

ChangeLog:
 -2025_12_31:
   Bootloader Example 
    - Fix Keil Example
	- Removed Timeout from DFU to simplify and make it more robust in case of errors
	- Fix index issue with unaligned DFU Data
   Application Example
    - Fix Keil Example
	- Updated to new RDM Library API
 -2025_03_18:
	Bootloader Example 
	- Removed the defines from project preprocessor because it was hard to recognize
	- Moved necessary defines in the dfu_update.h
	- Changed Buffer size for SPI DMA to 520 Bytes to make it possible to receive 512 Bytes DMX
	Application Example
	- Fix bug with dmx startaddress in example
    - Improve Example handling with SPI Library for support for crmx
    - Receive 512 Bytes
	- Increase Heap Size to 0x300
 -2024_11_08
	Bootloader Example
	- Added timeout if transfer has started (Major Bugfix)