Solution 
for Example II: Configuration Calculation (Self Test)
Pixel Calculation
· Color 1 (Beam): 1
· Color 2 (Wash): 20
· White: 15
· Pan: 1
· Tilt: 1
· Zoom: 20
Total configured Pixels: 58
Max allowed Pixels: 66
→Pixel Count within limit 



Static Block Calculation
· Color 1 (Beam) (Individual): 3
· Color 1 (Beam) (Shared): 1 (Master Strobe)
· Color 2 (Wash) (Individual): 0
· Color 2 (Wash) (Shared):  0
· White (Individual): 0
· White (Shared):  1 (White Strobe)
· Pan: 1
· Pan Endless Rotation: 1
· Tilt: 1
· Tilt Endless Rotation: 1
· Zoom: 1
· Focus: 1
· Frost: 1
· Prisma: 1
· Iris: 1
Total configured Static Blocks: 14
Max allowed Static Blocks: 12
→ Static Blocks not within limit 


FX Block Calculation
· Color 1 (Beam) (Individual): 8
· Color 1 (Beam) (Shared): 1 (Master Intensity)
· Color 2 (Wash) (Individual): 3
· Color 2 (Wash) (Shared):  0
· White (Individual): 1
· White (Shared):  0
· Pan: 1
· Pan Endless Rotation: 0
· Tilt: 1
· Tilt Endless Rotation: 0
· Zoom: 1
· Focus: 0
· Frost: 0
· Prisma: 0
· Iris: 0
Total configured FX Blocks: 16
Max allowed FX Blocks: 17
→ Static Blocks within limit 

→ Result: Configuration is not valid for nRF52833. The fixture needs the nRF52840, since in the nRF52840 there can be configured up to 24 Static Blocks.



